ASANA — SCAN-TO-CAD DELIVERABLES (v1, 2026-07-02)
==================================================
All content extracted from the site laser scans (E57), registered to the Metec/GA project grid (mm).
This is v1 — the QA-passed set. Plans, sections and slice ladders follow in v2 (in production).

CONTENTS
  ASA-SCAN-L03-HGT-01 Soffit Heights.pdf    L3 soffit height above floor, colour map + stats
                                            (median 3625mm; architect stated 3640 — verify datums)
  ASA-SCAN-L08-HGT-01 Soffit Heights.pdf    L8 structural soffit (measured through removed ceiling
                                            tiles, ~84% coverage; blank cells = no sightline, NOT low)
  ASA-SCAN-L03-FIT-01 ... Verification.pdf  As-built vs GA fit check. HEADLINE: built form fits the GA;
                                            overlay registration carries ~0.57deg trend (see verdict) —
                                            re-register on 3 spread targets before dimensional sign-off.
                                            Flags: 2 as-built columns with no GA column nearby (C02, C04)
                                            + a twin at C15 — verify on site.
  ASA-SCAN-*-UNDERLAY-*.dxf/.dwg            Native CAD point underlays (insert at 0,0, mm, 1:1):
                                            L03 high-level services / L03 low-level / L08 ceiling-void
                                            services. Points are snappable; PDMODE preset.

HONESTY NOTES
  - As-scanned capture: absence of points != absence of kit (occlusion shadows behind columns/walls).
  - L8 high-level = seen through ceiling tile gaps — real but patchy; blank != empty.
  - Registration residual ~50-60mm; see the FIT sheet before relying on absolute positions.
